Site Sign-Off Checklist

Checklist Type: Joinery

Project Name / Block: abinash

Apartment / Unit: jshg

Date of Inspection: 2025-05-15

Subcontractor Name: khdvhkfbvk

CH Foreman: hdfgvikegui

# Checklist Items

❌ Entrance door installed, plumb, and square

✅ Fire rating label visible and undamaged

✅ Intumescent seals fitted correctly (frame or door as required)

✅ Gap tolerances compliant and packers fitted correctly

❌ Door closes fully and latches without resistance

❌ Door furniture/ironmongery fitted to spec

✅ Entrance door liner installed straight and securely fixed

❌ Pod door flat liner fitted correctly and square

✅ Internal doors installed correctly with consistent gaps

❌ Hinges, handles, and latches fitted securely

❌ Skirting fitted tight to wall, level, and flush

❌ Joints (mitres, scribes) tight and filled where required

❌ Fixings fitted neatly

✅ Architraves fitted tight to frame and wall

❌ Consistent margins and clean mitres

❌ No gaps, damage, or poor cuts visible

✅ Correct type and size of thresholds installed

✅ Fitted level and securely fixed

❌ No sharp edges, trip hazards, or gaps

❌ Doorstops fitted correctly

✅ All ironmongery installed to spec

❌ Function tested – doors open, close, and latch smoothly with receivers adjusted

❌ No missing screws or loose components

✅ Damaged/missing components reported

❌ Area left tidy and safe

❌ Installation ready for inspection/handover

Subcontractor Signature:

